{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["english","deutsch"],"not_rendered":{"images":2,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"english","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"merged":[[5,0,5,5]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
["Daily Noise Exposure Level Post Processing Form V1.01"]
["Calculates the noise exposure level LEX,8h at steady noise with stepwise level variations"]
[]
["1. Measure the LAeq at the different sound levels"]
["2. Enter the LAeq results and the corresponding exposure time in the table below."]
[]
[]
[]
[null,"Nr.","Description","Exposure Time [hours]","Level LAeq [dB]"]
[null,1,"e.g. work at machine 1",{"v":6,"d":"6.00"},83.2]
[null,2,"e.g. work at machine 2",{"v":2,"d":"2.00"},80.4]
[null,3]
[null,4]
[null,5]
[null,6]
[null,7]
[null,8]
[null,9]
[null,10]
[]
[{"$nulls":3},"Sum Exposure Time [hours]","LEX,8h"]
[{"$nulls":3},{"v":8,"d":"8.00"},{"v":82.65075407663332,"d":"82.7"}]

{"sheet":"deutsch","index":1,"n_rows":27,"n_cols":5,"rows_kept":27,"merged":[[5,0,5,5]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
["Berechnung des Lärmexpositionspegel V1.01"]
["Berechnet den Lärmexpositionspegel LEX,8h bei unterschiedlichen Pegeln während der Arbeitszeit"]
[]
["1. Messen Sie die verschiedenen Schallpegel LAeq"]
["2. Füllen Sie die LAeq-Messwerte mit den jeweiligen Expositionszeiten in das Formular unten."]
[]
[]
[]
[null,"Nr.","Beschreibung der Tätigkeit","Expositionszeit [Stunden]","Schallpegel LAeq [dB]"]
[null,1,"z.B. Arbeit an Maschine 1",{"v":6,"d":"6.00"},83.2]
[null,2,"z.B. Arbeit an Maschine 2",{"v":2,"d":"2.00"},80.4]
[null,3]
[null,4]
[null,5]
[null,6]
[null,7]
[null,8]
[null,9]
[null,10]
[]
[{"$nulls":3},"Summe Zeit [Stunden]","LEX,8h"]
[{"$nulls":3},{"v":8,"d":"8.00"},{"v":82.65075407663332,"d":"82.7"}]